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SPEC. of XENO® High-Power LED Al-Alloy Flashlight
G42 V2/2013 XM-L2 with XENO HDDu 3+3 Engine
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Tested with 18650 battery: Panasonic 3400mAh // X061813ANS1074203EK by Kevin/XENO, Shenzhen, Summer 2013




XENO Co.  No.:X061813FS074203E

1. Brand: XENO®
Model No.: G42
Version: V2/2013 XM-L2
*.Datasheets under ANSI/NEMA FL-1 Standard:
1/. Light Output:715lms
2/. Runtime:1.5hrs at High Output level;150hrs at Ultra-Low level
3/. Beam Distance:320m
4/. Peak Beam Intensity:26000cd
5/. Impact Resistance:1m
6/. Water Resistance:IPX-8,10m
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2.Key Words:
1/.XENO HDDu 3+3 Engine inside:

   1//.Two Stand-Alone Closed Circulating Regulative System in HDDu 3+3:

      Normal:3-stage normal illumination variable output: High,Low,Ultra-Low

      Hidden:3-stage functional variable output: Strobe,LB(Locator Beacon),SOS

   2//.Linear regulative mode for variable output, Not the PWM mode

      Non-Flickering & Absolutely Noiseless even at Ultra-Low level.

      Rated Input:DC3.0~6V;

      Battery: Use 18650*1 Li-ion rechargeable battery or CR123A*2

   3//.Max Output: OTF715lms / Max Burning Time:150 hours
2/.CREE XM-L2 series LED, 1C U2,Cool White.

3/.Integral Design of head and body:
 Greatly improve the ability of Radiating, Waterproof and Dust-proof.
    Prevent accident loosen the head-cap while change the battery.

4/.Finished: Military Spec. Type III Hard-Anodized Al-Alloy Construction; Gun Grey.

5/.AR Lens: Ultra clear lens with Anti-Reflection coatings on both sides.

6/.XENO GR2: SIR (Silicone Rubber) Combat Grip, XENO new generation enhanced version.

7/.XENO unique Belt Clip BC2:

Detachable for clip maintenance.

High powered & flexibility enhanced, High reliability Belt Clip with 3D designing.

Qualified by 96 hours Salt Spray Test.

3. Features:
1/. XENO HDDu 3+3 Engine:

Two Stand-Alone Closed Circulating Regulative System in HDDu:

Normal:3-stage normal illumination variable output: High, Low, Ultra-Low

Hidden:3-stage functional variable output: Strobe, LB(Locator Beacon),SOS

Variable output and operations:

1//.Press to turn ON/OFF and soft click the button for variable output.

2//.Fast click(half press) no less than 3 times at any illumination output, you will get the functional output.

3//.Single click for next stage output  in both of two Stand-Alone Closed Circulating Regulative System in HDDu.

4//.High-Level is always the start-mode after more than 3 seconds light off from any output.
Linear LED driver, Not PWM mode.

Non-Flickering and Absolutely Noiseless even at Ultra-Low level.
With Ultra-Low output, more than 100 hrs burning time.

XENO unique Quiet RSL™ technology.

XENO unique GFC(Gamble Free Concept) impact-resistant technology.

Rated Input:DC3.0~6V;

Battery: Use 18650*1 Li-ion rechargeable battery or CR123A*2
Built-in battery inverted-load protection.

Built-in battery overdischarge protection.

Max Output: 715lms@2200mA(OTF, full high level)

Max Burning Time:150 hours@20mA(Ultra-Low level)
2/.Reflector:XENO precision aluminum long-throw reflector, SMO.
3/.AR Lens:
Ultra clear lens with Anti-Reflection coatings on both sides.

High quality toughened mineral-glass, precision polish the edge for impact-resistant.
4/.
Switch: The tactically-forward click tailcap switch, with XENO Silver contacts.
Support tail-standing ability.

5/.Water proof:IPX-8; 1 meters dunk-resistance.
6/.XENO GFC impact-resistant system:

Double Spring between anode “+” and cathode “-” of the battery for shock proof.

Both spring are 24K-Gold-Electroplate.

LED driver with XENO GFC impact-resistant technology

Shock isolation constructions for LED driver

7/. Enclosed XENO Genuine Accessory System:

XENO STT10:stainless Strike Bezel in tailcap: secure-ring, windows break, self-defence.
XENO RG42 Stainless Secure-Ring for Window(Lens).

XENO LS10E Enhanced Lanyard System, with XENO XRD-the best Lanyard Ring on the blue Earth.
XENO L01 Nylon Cord Wrist Lanyard
8/.Fits XENO Genuine Accessory System well(Optional):

XENO TW42–-Diffuser/Traffic Wand/XENO IGO

XENO HD42—the most reliable holster on the blue Earth/XENO IGO

4. Specifications

1/.Emitter: CREE High-Power LED,XM-L2 series:

XM-L2 1C U2,CT5000~8300K,CoolWhite,MaxOutput 715lms;

2/.Rated Input: DC3.0~6V;

Battery: Use 18650*1 Li-ion rechargeable battery or CR123A*2
3/.Output (Cool White version; Related current, OTF lumens, burning time):
Normal: 3-Stage Normal Illumination Variable Output:

High (715lms/1.5hrs),
Low (390lms/4hrs),
Ultra Low (13lms/150hrs)

Hidden: 3-Stage Functional Variable Output:

Strobe (4.5hrs @ high level output),
LB (18hrs @ low level output),
SOS (9hrs @ low level output).

*The experience result will be a little different for the battery of different brand, condition etc.
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5.Size & Weight:

Size:length 6.3’’(160mm), Ø1.8’’(Ø46.5mm,bezel).
Battery tube:1’’(25.4mm)

N.W.: 7.5 oz(212g,battery not included).

Packing:XENO CP02 color box;
Size:L162*W56*H63.5mm;G-Weight: 9.7 oz (275g).
XENO Co  www.xenoled.com
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